IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Numéro du projet"
Time stamp: "2018-04-16T10:45:31"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140606_1530(x64) - Exporter 2015.0.2014.0606 - Default UI"
Application: "Autodesk Revit LT 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit LT 2015 (ENU)"

People and organizations
  Person "Yohann.Dacosta" of Organization (no name given)
  Owner history of Person "Yohann.Dacosta" of Organization (no name given) | application "Autodesk Revit LT 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit LT 2015 (ENU)" | change NOCHANGE | created 1521563971 (2018-03-20T16:39:31Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Numéro du projet" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 52′ 0.117187″ | longitude 2° 19′ 59.880409″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCSLAB | object type "Floor:QUALITOP METAL" | FLOOR | names: "Floor:QUALITOP METAL:126741" | material: layers "Floor:QUALITOP METAL" ("QUALITOP METAL - White cement - White" 2., "Concrete" 10.9, "Steel Mesh" 0.6, "Concrete" 1.5, "Sub base" 20.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Other, Phasing

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "QUALITOP METAL" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "RCR" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Level = "Level: Niveau 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 1. (IFCAREAMEASURE) [SQUARE_METRE]
    Perimeter = 400. (IFCLENGTHMEASURE) [CENTI METRE]
    Thickness = 35. (IFCLENGTHMEASURE) [CENTI METRE]
    Volume = 0.35 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Propriétaire" (IFCTEXT)
    Project Address = "Entrer l'adresse ici" (IFCTEXT)
    Project Issue Date = "Date de fin" (IFCTEXT)
    Project Name = "Nom du projet" (IFCTEXT)
    Project Number = "Numéro du projet" (IFCTEXT)
    Project Status = "Etat du projet" (IFCTEXT)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: QUALITOP METAL" (IFCLABEL)
    Family and Type = "Floor: QUALITOP METAL" (IFCLABEL)
    Type = "Floor: QUALITOP METAL" (IFCLABEL)
    Type Id = "Floor: QUALITOP METAL" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Pointe 8 mm" (IFCLABEL)
    Family and Type = "Level: Pointe 8 mm" (IFCLABEL)
    Type = "Level: Pointe 8 mm" (IFCLABEL)
    Type Id = "Level: Pointe 8 mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCSLAB)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Niveau 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CE marking = "CT - C80 F10 A 3/ AR 0.5" (IFCTEXT)
    Description = "Qualidur High Performance is a factory blend" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "RCR" (IFCTEXT)
    Model = "Qualitop Metal" (IFCTEXT)
    Product code = "RCR-001" (IFCTEXT)
    Standard = "EN13813 : Screed materials" (IFCTEXT)
    Type Comments = "Medium to heavy duty floor hardener" (IFCTEXT)
    Type Name = "QUALITOP METAL" (IFCTEXT)
    URL = "http://www.rocland.eu/en/product/hardeners/111-qualitop-metal.html" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Pointe 8 mm" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties | properties | on 1 object (1 IFCSLAB)
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 35. (IFCLENGTHMEASURE) [CENTI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Data | properties | on 1 object (1 IFCSLAB)
    Abrasion resistance = "A3" (IFCTEXT)
    Application = "Qualitop METAL should be spread evenly on the surface at a rate of 2 to 6-8kg/m²" (IFCTEXT)
    Application recommendation = "The curing agent Roc Cure 60 or ECOCURE 17 should be applied immediately after the finishing operation is complete" (IFCTEXT)
    Compressive strength = "≥ 80 N/mm² (C80)" (IFCTEXT)
    Flexural strength = "≥10N/mm² (F 10)" (IFCTEXT)
    LEED = "VOC 2gr/l - VOC limit is 100 g/l" (IFCTEXT)
    Nominal consumption by dry shaking = "6-8 kg/m²" (IFCTEXT)
    Nominal consumption by mechanical spreader = "6-8 kg/m²" (IFCTEXT)
    Nominal consumption by ‘fresh on fresh’ topping = "" (IFCTEXT)
    Reaction to fire = "A1fl" (IFCTEXT)
    VOC = "2g/l (limit 100g/l)" (IFCTEXT)
  General | properties | on 1 object (1 IFCSLAB)
    CSTB certification = "15-26054936" (IFCTEXT)
    Data sheet = "http://www.rocland.eu/en/wp-content/uploads/2014/05/uk_ft_qualitop_metal.pdf" (IFCTEXT)
    Leed confirmation = "http://www.rocland.eu/en/wp-content/uploads/2014/05/LEED-certificat-A-EN.pdf" (IFCTEXT)
    Safety Data Sheet = "http://www.rocland.eu/en/wp-content/uploads/2013/12/uk-fds-qualitop-metal.pdf" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCSLAB)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Marqueur de niveau - Cercle: Marqueur de niveau - Cercle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCSLAB)
    Structural Material = "Concrete" (IFCLABEL)