IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Numéro du projet"
Time stamp: "2018-03-20T17:48:24"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140606_1530(x64) - Exporter 2015.0.2014.0606 - Default UI"
Application: "Autodesk Revit LT 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit LT 2015 (FRA)"

People and organizations
  Person "Yohann.Dacosta" of Organization (no name given)
  Owner history of Person "Yohann.Dacosta" of Organization (no name given) | application "Autodesk Revit LT 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit LT 2015 (FRA)" | change NOCHANGE | created 1521563970 (2018-03-20T16:39:30Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Numéro du projet" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 52′ 0.117187″ | longitude 2° 19′ 59.880409″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCSLAB | object type "Floor:QUALIDUR HP" | FLOOR | names: "Floor:QUALIDUR HP:126741" | material: layers "Floor:QUALIDUR HP" ("QUALIDUR HP - Ciment blanc - Blanc" 2., "Béton" 10.9, "Nappe armature" 0.6, "Béton" 1.5, "Fond de forme" 20.) | property sets: Pset_SlabCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Other, Phasing

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "QUALIDUR HP" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSLAB)
    Manufacturer = "RCR" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Level = "Level: Niveau 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 1. (IFCAREAMEASURE) [SQUARE_METRE]
    Perimeter = 400. (IFCLENGTHMEASURE) [CENTI METRE]
    Thickness = 35. (IFCLENGTHMEASURE) [CENTI METRE]
    Volume = 0.35 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Propriétaire" (IFCTEXT)
    Project Address = "Entrer l'adresse ici" (IFCTEXT)
    Project Issue Date = "Date de fin" (IFCTEXT)
    Project Name = "Nom du projet" (IFCTEXT)
    Project Number = "Numéro du projet" (IFCTEXT)
    Project Status = "Etat du projet" (IFCTEXT)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: QUALIDUR HP" (IFCLABEL)
    Family and Type = "Floor: QUALIDUR HP" (IFCLABEL)
    Type = "Floor: QUALIDUR HP" (IFCLABEL)
    Type Id = "Floor: QUALIDUR HP" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Pointe 8 mm" (IFCLABEL)
    Family and Type = "Level: Pointe 8 mm" (IFCLABEL)
    Type = "Level: Pointe 8 mm" (IFCLABEL)
    Type Id = "Level: Pointe 8 mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCSLAB)
    Phase Created = "Phase 1" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Niveau 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code du produit = "RCR-001" (IFCTEXT)
    Description = "Durcisseur à haute performance" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "RCR" (IFCTEXT)
    Marquage CE = "CT - C70 F10 A 3/ AR1" (IFCTEXT)
    Model = "Qualidur HP" (IFCTEXT)
    Norme = "EN13813 : Matériaux pour chapes" (IFCTEXT)
    Type Comments = "Couche d’usure à haute dureté pour les sols industriels monolithiques soumis aux trafics sévères" (IFCTEXT)
    Type Mark = "ROCLAND" (IFCTEXT)
    Type Name = "QUALIDUR HP" (IFCTEXT)
    URL = "http://www.rocland.eu/fr/rocland/produits/durcisseurs/218-qualidur-hp.html" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Pointe 8 mm" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties | properties | on 1 object (1 IFCSLAB)
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 35. (IFCLENGTHMEASURE) [CENTI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Data | properties | on 1 object (1 IFCSLAB)
    Application = "Le dosage du durcisseur doit être de 4-5kg/m² - 2mm" (IFCTEXT)
    COV = "2g/l (limite 100g/l)" (IFCTEXT)
    Consommation nominale par chape incorporée (coulis) = "12 kg/m²" (IFCTEXT)
    Consommation nominale par épandage manuel = "4-5 kg/m²" (IFCTEXT)
    Consommation nominale par épandage mécanique (Spreader) = "4-5 kg/m²" (IFCTEXT)
    LEED = "VOC 2gr/l - VOC limit is 100 g/l" (IFCTEXT)
    Recommandation d'application = "Le produit de cure Roc Cure 60, Ecocure 17, Ecocure Superior ou Roc Seal premium doivent être Pulvérisés immédiatement après les travaux de finition sur l’intégralité de la surface." (IFCTEXT)
    Réaction au feu = "A1fl" (IFCTEXT)
    Résistance à l'abrasion = "A3" (IFCTEXT)
    Résistance à la compression = "≥ 70 N/mm² (C70)" (IFCTEXT)
    Résistance à la flexion = "≥10N/mm² (F 10)" (IFCTEXT)
  General | properties | on 1 object (1 IFCSLAB)
    Certificat CE = "http://www.rocland.eu/fr/wp-content/uploads/2014/05/fr_dop_qualidur-hp.pdf" (IFCTEXT)
    Certification CSTB = "15-26055645/2" (IFCTEXT)
    Fiche de sécurité = "http://www.rocland.eu/fr/wp-content/uploads/2014/05/fr-fds-rocland1.pdf" (IFCTEXT)
    Fiche technique = "http://www.rocland.eu/fr/wp-content/uploads/2014/05/fr_ft_qualidur_hp.pdf" (IFCTEXT)
    PV CSTB = "http://www.rocland.eu/fr/wp-content/uploads/2014/05/fr_cstb_qualidur.pdf" (IFCTEXT)
    Recommandations utiles = "Les variations de teinte sur les sols industriels à base de liant hydraulique sont inévitables" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCSLAB)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Marqueur de niveau - Cercle: Marqueur de niveau - Cercle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCSLAB)
    Structural Material = "Béton" (IFCLABEL)